* A displacement detection method based on Bayesian inference from GNSS kinematic positioning is presented.
* A new probability model of displacement detection is developted.
* Bayesian inference is implemented by Markov Chain Monte Carlo sampling
* Displacement detection is achieved by posterior samples of parameters